For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Stabilizer Shaft Clamp Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Stabilizer Shaft Insulator Clamp (Qty: 2)
3 | Stabilizer Shaft Insulator (Qty: 2) Tip Lift up on the stabilizer shaft to gain enough clearance to remove the insulator.