For 1990-2009 cars

## Quarter Upper Trim Panel Replacement with TB5

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the seat belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Rear Quarter Upper Trim Panel Screw Caution: Refer to Fastener Caution in the Preface section. Tip Open the access door to remove screw. Tighten
3 N·m (27 lb in)

2 | Rear Quarter Upper Trim Panel Assembly Tip Route the seat belt through the trim panel.

## Quarter Upper Trim Panel Replacement without TB4

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the seat belt anchor bolt. Refer to Rear Seat Number 2 Retractor Side Belt Replacement.

1 | Rear Quarter Upper Trim Panel Screw Caution: Refer to Fastener Caution in the Preface section. Tip Open the access door to remove screw. Tighten
3 N·m (27 lb in)

2 | Rear Quarter Upper Trim Panel Clip (Qty: 3)
3 | Rear Quarter Upper Trim Panel Retainer
4 | Rear Quarter Upper Trim Panel Assembly Tip Route the seat belt through trim panel.