For 1990-2009 cars

### RUST THROUGH PERFORATION REPAIRS

Labor operations in this section are to be used for the repair of rust through perforation damage. All labor operations listed below allow 1.5 hours of labor time and should be entered as Regular Labor Hours. In the event the rust through damage is extensive enough to require panel replacement, the labor time required to replace the panel should be submitted as straight time (ST) in the Other Labor Hours column and appropriate authorization is required. Refer to the Paint section of this guide for paint times and enter the paint time as Regular Labor Hours.

Note: Refer to the appropriate GM publication for claims processing guidelines.

S5070 | Hood -- Corrosion Perforation Repair
S5090 | Fender -- Corrosion Perforation Repair
S5150 | Pillar, Windshield -- Corrosion Perforation Repair
S5170 | Roof -- Corrosion Perforation Repair
S5190 | Pillar, Center -- Corrosion Perforation Repair
S5210 | Rocker -- Corrosion Perforation Repair
S5250 | Door, Front -- Corrosion Perforation Repair
S5252 | Door, Rear -- Corrosion Perforation Repair
S5254 | Door, Sliding -- Corrosion Perforation Repair
S5310 | Pickup Cab Rear -- Corrosion Perforation Repair
S5350 | Rear Quarter -- Corrosion Perforation Repair
S5410 | Pickup Box -- Corrosion Perforation Repair
S5450 | Rear Compartment Door/ Lid/Liftgate/Endgate -- Corrosion Perforation Repair