For 1990-2009 cars

#### Special Tools

EN-46104 Water Pump Pulley Holding Tool

For equivalent regional tools, refer to Special Tools.

1. Ensure that the engine front cover and water pump are clear of old gasket material.
2. Place a new water pump gasket on the water pump.
3. Place the water pump in position on the front cover.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the water pump bolts and tighten to 10 N·m (89 lb in).
5. Install the water pump pulley.
6. Loosely install the water pump pulley bolts.
7. Install the EN-46104 tool (1) onto the water pump pulley and tighten to 10 N·m (89 lb in).