For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.

1 | Front Side Door Speaker Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Front Side Door Speaker

#### Procedure

Disconnect the electrical connectors.