For 1990-2009 cars

## Front Fender Upper Rear Molding Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the front driver or passenger door in order to access the retainers.

1 | Front Fender Upper Rear Molding Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Integral Retainer Clip (Qty: 3)
3 | Front Fender Upper Rear Molding Assembly

#### Procedure

1. Remove the screw.
2. Carefully release the three retainers from the front fender upper rear molding and release four retainers from the forward edge of the front and rear upper reveal molding.
3. Hold onto the front and rear side door upper reveal molding and pull the front fender upper rear molding butt joint apart.