For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the right and left rear wheelhouse. Refer to Rear Wheelhouse Panel Liner Replacement.

1 | Rear Fascia Bolt (Qty: 2)
2 | Rear Fascia Retainers (Qty: 2)
3 | Rear Fascia Bolt Cover (Qty: 24)
4 | Rear Bumper Fascia Screw (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
5 | Rear Fascia

#### Procedure

• | Disconnect the electrical connectors/harnesses as needed.

• | Transfer any parts as needed.