For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: In order to avoid actuator damage, DO NOT apply power to the actuator when it is not installed in the HVAC module.

#### Preliminary Procedures

1. Remove the right rear quarter trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the rear wheelhouse liner panel. Refer to Rear Wheelhouse Panel Liner Replacement.
3. Remove the HVAC module mounting nuts and reposition the auxiliary HVAC module inward to gain access to the mode door actuator.
4. Disconnect the electrical connector from the mix door actuator.

1 | Mode Door Actuator Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (16 lb in)
2 | Auxiliary Mode Door Actuator

#### Procedure

Re-calibrate the mode actuator. Refer to Actuator Recalibration.