For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console accessory trim plate. Refer to Front Floor Console Accessory Trim Plate Replacement.
2. Remove the right and left front floor console fillers. Refer to Front Floor Console Filler Replacement.

1 | Front Floor Console Armrest Assembly Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Front Floor Console Armrest Assembly

#### Procedure

Position the armrest assembly out of the way leaving the electrical harness attached.

3 | Front Floor Upper Console Trim Plate

#### Procedure

Lift the rear of the trim plate first, releasing the retainers securing the trip plate to the console assembly.

4 | Retainer Clips (Qty: 4)