For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Remove the foam pad insulators, as required.

1 | Fuel Tank
2 | Evaporative Emission Canister Vent Front Pipe

#### Procedure

1. Disconnect the quick connect fitting from the evaporative emission canister. Refer to Plastic Collar Quick Connect Fitting Service .
2. Disengage from the tank retaining features.