For 1990-2009 cars

## Liftgate Upper Molding Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the liftgate in order to access the applique integral tabs and retainers.

1 | Integral Tabs (Qty: 6)
2 | Liftgate Applique

#### Procedure

Release the retainers and roll the applique outward off from the hem flange.

## Liftgate Upper Molding Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the liftgate in order to access the applique integral tabs and retainers.

1 | Integral Tab (Qty: 6)
2 | Liftgate Applique

#### Procedure

Release the retainers and roll the applique rearward off from the hem flange.