For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Hinge Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Support the door before removing the hinge bolts.
3. Disconnect the electrical connector, if equipped.
4. With the aid of an assistant, remove the door.

Tighten
8 N·m (71 lb in)

2 | Rear Side Door Hinge Bolt (Qty: 2) Tighten 8 N·m (71 lb in)
3 | Rear Side Door Assembly Tip When replacing the door it is necessary to transfer all of the internal components.