For 1990-2009 cars

## Front and Rear Side Door Opening Frame Reveal Molding Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the front and rear door on the side the door opening frame reveal molding will be replaced.

1 | Front and Rear Side Door Opening Frame Reveal Molding Integral Clip (Qty: 12)
2 | Front and Rear Side Door Opening Frame Reveal Molding

#### Procedure

1. Remove the front fender upper rear molding. Refer to Front Fender Upper Rear Molding Replacement.
2. Carefully release the front frame reveal molding from the butt joint located at the quarter panel bezel joint tie plate.
3. Upon installation, secure the butt joint ends firmly together prior aligning the molding retainer clips to the body panel.
4. Secure the front fender upper rear molding. Refer to Front Fender Upper Rear Molding Replacement.