For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the window regulator. Refer to Front Side Door Window Regulator Replacement or Rear Side Door Window Regulator Replacement.

1 | Door Window Regulator Motor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (9 lb in)
2 | Door Window Regulator Motor Stud Bolt Tighten 5 N·m (9 lb in)
3 | Door Window Regulator Motor

#### Procedure

Reprogram the window motor. Refer to Control Module References.