For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Outer Sealing Strip Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Rear Side Door Outer Sealing Strip

#### Procedure

1. Remove by lifting up on seal starting at the rear and working forward.
2. When re-installing, align outer seal fastener location with hole in door structure and outer panel retaining tabs.
3. Start at rear of belt seal, push down onto flange until fully seated.