For 1990-2009 cars

## Door Lock and Side Window Switch Replacement - Passenger Side Outlook with RPO AXA

Callout | Component Name
--- | ---
1 | Front Side Door Lock and Side Window Switch Plate

#### Procedure

Use a flat-bladed tool to pry the switch plate from the door handle assembly.

2 | Front Side Door Lock Switch

#### Procedure

Disconnect the electrical connector.

3 | Front Side Door Window Switch

#### Procedure

Disconnect the electrical connector.

## Door Lock and Side Window Switch Replacement - Passenger Side with RPO AXE or AXC

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the passenger side door trim panel. Refer to Front Side Door Trim Panel Replacement - Right Side.

1 | Front Side Door Lock and Side Window Switch Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Front Side Door Lock and Side Window Switch Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Refer to Control Module References for programming and set-up information.

## Door Lock and Side Window Switch Replacement - Passenger Side Enclave with RPO AXE or AXC

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the passenger side door trim panel. Refer to Front Side Door Trim Panel Replacement - Right Side.

1 | Front Side Door Lock and Side Window Switch Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Front Side Door Lock and Side Window Switch Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Refer to Control Module References for programming and set-up information.