For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .

1 | Power Steering Reservoir Inlet Hose Clip
2 | Power Steering Reservoir Inlet Hose Clamp (Qty: 2)

#### Procedure

1. Remove as much power steering fluid from the remote power steering fluid reservoir as possible.
2. Place drain pans under the vehicle as needed.

3 | Power Steering Reservoir Inlet Hose

#### Procedure

1. Clean any excess fluid from the vehicle and remove the drain pans.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding .