For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement.

1 | Liftgate Handle Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Liftgate Handle Assembly

#### Procedure

1. Remove the rearview camera, if equipped. Refer to Rearview Camera Replacement.
2. Disconnect the electrical connector.