For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear speaker grille. Refer to Radio Rear Speaker Grille Replacement.

1 | Radio Rear Quarter Trim Speaker Assembly Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Rear Quarter Trim Speaker Assembly

#### Procedure

Disconnect the electrical connector.