For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the left rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.

1 | Rear Body Control Module Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Reprogram the rear body control module if replaced. Refer to Control Module References.

Tip
Push in the tab to release the module from the liftgate actuator assembly.