For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

It is only necessary to lower the headliner. Only do those step in headliner replacement that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement.

1 | Sunroof Sunshade Motor/Actuator Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tip
When removing the sunroof motor/actuator the cables and tubes stay with the module.

Tighten
3 N·m (27 lb in)

2 | Sunroof Sunshade Motor/Actuator

#### Procedure

Initialization/Teach motor/actuator, refer to Sunroof Motor/Actuator Initialization/Teach Process.