For 1990-2009 cars

## Front Bumper Fascia Emblem Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia in order to access and remove the heat stakes from the emblem assembly. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Fascia Emblem Assembly

#### Procedure

1. Place the front bumper fascia face down on a clean protected surface.
2. Cut the heat stakes from the rear side of the emblem assembly.
3. Remove the emblem from the bumper fascia.
4. Place the new emblem locator pins to the holes in the front bumper fascia.
5. Hold the emblem firmly against the front bumper fascia.

2 | Front Bumper Fascia Emblem Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten Hand Tighten the nuts.