For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the right front wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement.
3. Remove the intermediate drive shaft mounting bolts from the engine bracket.
4. Remove the intermediate drive shaft from the vehicle.

### Installation Procedure

1. Install the intermediate drive shaft to the transaxle.
2. Position the intermediate shaft support bracket to the engine.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the support bracket bolts.

Tighten
Tighten the bolts to 58 N·m (43 lb ft).

4. Install a new wheel drive shaft retaining ring.
5. Install the right wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement.
6. Remove the support and lower the vehicle.