For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the radiator inlet hose. Refer to Radiator Inlet Hose Replacement.
2. Remove the right engine strut mount. Refer to Engine Mount Strut Replacement - Right Side.
3. Remove the right engine mount strut bracket. Refer to Engine Mount Strut Bracket Replacement - Right Side.

1 | Water Outlet Housing Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the water outlet housing bolts.

Tighten
10 N·m (89 lb in)

2 | Water Outlet Housing
3 | Seal

#### Procedure

1. Remove the water outlet housing seal. Discard the seal.
2. Install a new water outlet housing seal.