For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the liftgate actuator (if equipped). Refer to Liftgate Actuator Replacement .

1 | Communication Interface Module Bracket

#### Procedure

1. Disconnect the body harness from the bracket as required.
2. Loosen the bracket fasteners to remove the bracket from the slotted holes.
3. Disconnect the electrical connectors.

2 | Rear Object Alarm Module