For 1990-2009 cars

## Instrument Cluster Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Replacement.

1 | Instrument Panel Cluster Trim Plate Spacer Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Instrument Panel Cluster Trim Plate Spacer
3 | Instrument Panel Cluster Assembly Screw (Qty: 2) Tighten 2.5 N·m (22 lb in)
4 | Instrument Panel Cluster Assembly

#### Procedure

1. Disconnect the electrical connections.
2. After replacing the instrument panel cluster, remove the instrument panel cluster fuse for a few seconds and then install the fuse.
3. Refer to Control Module Referencesfor programming and setup information

## Instrument Cluster Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Replacement.

1 | Instrument Panel Cluster Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Assembly Procedure

1. Disconnect the electrical connector.
2. After replacing the instrument panel cluster, remove the instrument panel cluster fuse for a few seconds and then install the fuse.
3. Refer to Control Module References for programming and setup information.

## Instrument Cluster Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument cluster trim plate assembly. Refer to Instrument Panel Cluster Trim Plate Replacement.

1 | Instrument Cluster Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Cluster Assembly

#### Procedures

1. Disconnect the electrical connections.
2. After replacing the instrument panel cluster, remove the instrument panel cluster fuse for a few seconds and then install the fuse.
3. Refer to Control Module References for programming and setup information.

## Instrument Cluster Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument cluster trim plate applique. Refer to Instrument Panel Cluster Trim Plate Applique Replacement.

1 | Instrument Cluster Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Cluster Assembly

#### Procedure

1. Disconnect the electrical connections.
2. After replacing the instrument panel cluster, remove the instrument panel cluster fuse for a few seconds and then install the fuse.
3. Refer to Control Module References for programming and setup information.