For 1990-2009 cars

### Inspection Procedure

1. Inspect the capsules on the steering column bracket assembly. Verify that the capsules are seated securely in the bracket slots and inspect the capsules for any loose conditions when pushed or pulled by hand. If the capsules are not secure, perform one of the following procedures:

• | If the bracket is bolted to the jacket assembly, replace the bracket.

• | If the bracket is welded to the jacket assembly, replace the jacket assembly.

2. Inspect the jacket assembly for collapse by measuring the distance from the lower edge of the upper jacket to a defined point on the lower jacket. If measured dimensions (A), are not within specifications (100 mm), install a steering column.