For 1990-2009 cars

1. Loosen the adjuster cam nut (1).
2. Using a wrench to rotate the adjuster bolt (2), adjust the cam (3) to specifications.

Caution: Refer to Fastener Caution in the Preface section.

Note: Ensure that the camber settings have not changed after torquing the adjuster nut to specifications. Readjust if necessary.

3. Using a wrench to hold the adjuster bolt (2), tighten the adjuster nut (1).

Tighten
Tighten the nut to 140 N·m (103 lb ft).

4. Check the toe alignment and adjust if required. Refer to Rear Toe Adjustment.
5. Test drive the vehicle.