For 1990-2009 cars

## Rear Wheel Bearing and Hub Replacement AWD

Callout | Component Name
--- | ---
Caution: The wheel bearing and hub assembly includes a magnetic encoder with built-in permanent magnets that the wheel speed sensor senses. Any contact with another magnet will damage the encoder magnets. The damage will cause a diagnostic trouble code to be set and will require wheel bearing and hub replacement.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear brake rotor. Refer to Rear Brake Rotor Replacement.

1 | Wheel Drive Shaft Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 205 N·m (151 lb ft)
2 | Wheel Bearing and Hub Bolt (Qty: 3)

#### Procedure

Using the J 42129 , separate the front wheel hub and bearing from the wheel drive shaft.

Tighten
140 N·m (103 lb ft).

#### Special Tools

J 42129 Front/Rear Spindle Remover

3 | Rear Wheel Bearing and Hub Assembly

## Rear Wheel Bearing and Hub Replacement FWD

Callout | Component Name
--- | ---
Caution: The wheel bearing and hub assembly includes a magnetic encoder with built-in permanent magnets that the wheel speed sensor senses. Any contact with another magnet will damage the encoder magnets. The damage will cause a diagnostic trouble code to be set and will require wheel bearing and hub replacement.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear brake rotor. Refer to Rear Brake Rotor Replacement.

1 | Rear Wheel Bearing and Hub Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 140 N·m (103 lb ft)
2 | Rear Wheel Bearing and Hub