For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel with Windshield Defroster Nozzle Grille Replacement.

1 | Head Up Display Module Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Head Up Display Module Assembly

#### Procedures

1. Disconnect the electrical connections.
2. Refer to Control Module References for programming and setup information.