For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left side trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.

1 | Liftgate Actuator Rod Warning: When a lift gate hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Procedure

1. Release the locking tabs on the actuator rod.
2. Calibrate the liftgate. Refer to Liftgate Calibration.