For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the right rear quarter trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
2. Remove the upper air temperature sensor, if equipped.

1 | Air Distribution Duct Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Lower Air Distribution Duct

#### Procedure

Squeeze both ends of distribution duct to release for removal.