For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear floor console right side trim panel. Refer to Rear Floor Console Side Trim Panel Replacement - Right Side.
2. Remove the rear floor console left side trim panel. Refer to Rear Floor Console Side Trim Panel Replacement - Left Side.

1 | Rear Floor Console Lid Trim Cover Screw (Qty: 14) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Lid Trim Cover
3 | Rear Floor Console Storage Lower Tray Screw (Qty: 4) Tighten 2.5 N·m (22 lb in)
4 | Rear Floor Console Storage Lower Tray Screw (Qty: 4) Tighten 2.5 N·m (22 lb in)
5 | Rear Floor Console Storage Lower Tray Assembly