For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Back Cushion Rear Finish Panel

#### Procedure

1. Using a flat bladed tool, from the side, push inward on one of the top retainers while pulling rearward at the top of the panel.
2. Release the clip on the opposite side.
3. Lift the panel upward to remove from the seat.

2 | Front Seat Head Restraint Assembly

#### Procedure

1. Push and hold the button on the left head restraint guide in to adjust the head restraint to the highest position.
2. Push the button on the right head restraint guide in while pulling upward to finish releasing the head restraint from the seat.

3 | Front Seat Head Restraint Guide (Qty: 2) Tip Use a rubber mallet or equivalent to tap upward on the bottom of the head restraint guide to remove from the seat back frame.