For 1990-2009 cars

## Front Side Door Emblem/Nameplate Replacement Acadia

Callout | Component Name
--- | ---
1 | Front Door Nameplate (GM)

#### Procedure

1. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
2. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the door, wipe the surface dry with a clean lint-free towel prior to installing the new GM nameplate.
3. Press the nameplate firmly to the front door molding to ensure full adhesion to the molding is made.

## Front Side Door Emblem/Nameplate Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Front Door Nameplate (GM)

1. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
2. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the door, wipe the surface dry with a clean lint-free towel prior to installing the new GM nameplate.
3. Press the nameplate firmly to the front door molding to ensure full adhesion to the molding is made.

## Front Side Door Emblem/Nameplate Replacement TRAVERSE

Callout | Component Name
--- | ---
1 | Front Side Door Nameplate Assembly (TRAVERSE)

#### Procedure

1. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
2. Use a J 25070 or equivalent and a small flat-bladed tool in order to remove the old letter nameplate.
3. Clean all the adhesive residue from the door bodyside molding, wipe the surface dry with a clean lint-free towel prior to installing the new TRAVERSE letter nameplate.
4. Close the front door.
5. Press the nameplate firmly to the front door molding to ensure full adhesion to the body side molding is made.

## Front Side Door Emblem/Nameplate Replacement Enclave GM

Callout | Component Name
--- | ---
1 | Front Side Door Nameplate/Emblem Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. The part and surface should be 21°C (70°F) prior to installation. The vehicle should remain 21°C (70°F) for one hour after assembly to allow adhesive to develop sufficient bond strength.
2. Use a J 25070 Heat Gun or equivalent to remove the old nameplate. Clean all the adhesive residue from the door and wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
3. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
4. Close the door prior to installing the new nameplate/emblem to the lower front rocker molding.
5. Remove the protective liner from the back side of the adhesive tape.
6. Align the nameplate/emblem to the front rocker molding and press to ensure full adhesion is made.