For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat No. 2 assembly. Refer to Rear Number 2 Seat Replacement.
2. Remove the rear seat No. 2 center belt assembly. Refer to Rear Seat Number 2 Belt Buckle Replacement.
3. Remove the rear seat No. 2 center buckle assembly. Refer to Rear Seat Number 2 Belt Buckle Replacement.

1 | Rear Seat No. 2 Riser Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat No. 2 Hinge Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Rear Seat No. 2 Riser Assembly

#### Procedure

Disconnect the cables from the seat riser.