For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat belt anchor finish cover.
2. Remove the front seat belt anchor plate bolt. Refer to Seat Belt Retractor Pretensioner Replacement - Front.

1 | Front Seat Adjuster Bolt Finish Cover Tip Use a small flat-bladed tool to release the tab in the rear of the cover.
2 | Front Seat Adjuster Bolt Finish Cover Tip Pull upward to release the retainer clip securing the cover to the seat adjuster.
3 | Front Seat Assembly Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
4 | Front Seat Assembly

#### Procedure

1. Disable the SIR. Refer to SIR Disabling and Enabling.
2. Lift the seat upward at the rear of the seat.
3. Disconnect the electrical connectors.
4. Slide the seat rearward to disengage the adjuster hooks holding the seat to the floor pan.