For 1990-2009 cars

### Removal Procedure

Notice: Be careful not to damage door sound insulator. Make sure all seals are properly positioned.

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement . The outer panel is removed in the illustration to show the location.
2. Remove the window. Refer to Rear Side Door Window Replacement .
3. Disconnect the harness from the power regulator.
4. Loosen the regulator bolts and slide the regulator assembly out of the door.

### Installation Procedure

1. Slide the regulator assembly into the door and position the regulator with the attachment bolts.
2. Install the window to the regulator assembly. Refer to Rear Side Door Window Replacement .
3. Install the wiring harness connector to the motor.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the regulator assembly bolts.

Tighten
Tighten the rear window regulator bolts to 10 N·m (89 lb in).

5. Check the regulator for proper operation.
6. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .