For 1990-2009 cars

### Removal Procedure

1. From under the vehicle, remove the front push pin from the wheelhouse liner.
2. Disconnect the wiring harness from the pump.
3. Place the holding container under the pump to catch the solvent from the container.
4. Disconnect the hose from the pump.
5. Remove the pump by pulling firmly.

### Installation Procedure

1. Install the pump by pushing firmly into the opening in the container.
2. Connect the hose to the pump.
3. Connect the wiring harness to the pump.
4. Install the front push pin to the wheelhouse liner.

Notice: Do not reuse washer fluid as debris may clog the system.

5. Fill the solvent container with washer solvent.