For 1990-2009 cars

## Coat Hook Replacement 1st Design

### Removal Procedure

Remove the coathooks by inserting a small screwdriver blade between the outside of the hook and the center section. Apply pressure to force the center section outward.

### Installation Procedure

1. Place the coathooks in the quarter window garnish moldings holes.
2. Once the hooks are seated in the spaceframe, push the center of the hooks in to lock it in place.

## Coat Hook Replacement 2nd Design

### Removal Procedure

1. Remove the coathook screw.
2. Remove the coathook.

### Installation Procedure

1. Position the coathook.
2. Install the screw.

Tighten
Tighten the coathook screw to 2.5 N·m (22 lb in).