For 1990-2009 cars

### Removal Procedure

1. Remove the rear washer fluid bottle as outlined in this section.

Notice: Do not reuse washer fluid as debris may clog the system.

2. Drain the contents of the bottle into a holding container.
3. Grasp the washer fluid pump and pull it out of the bottle.

### Installation Procedure

1. Lubricate the washer bottle grommet with soapy water or grease.
2. Insert the pump inlet spout into the rubber grommet.
3. Push the pump in until seated into the bottle.
4. Install the rear washer fluid bottle as outlined in this section.