For 1990-2009 cars

Replacement parts identified below by name, part number, or specification can be obtained from your dealer.

Part | Saturn Part Number
--- | ---
Air Cleaner Element - SOHC (L24) Engine or DOHC (LL0 ) Engine | 21000938
Surge Tank Pressure Cap | 10296465
Battery: The battery shield is designed for the size of the battery supplied withthe vehicle. Always replace the battery with the same size. (Battery life will be reduced if the battery shield is not used.)
Automatic Transaxle Filter | 21003361
Engine Oil Filter | 21000872
PCV Valve | 25147308
Fuel Filter | 21008344
Drive Belt: Automatically controlled by a tensioner

#### Windshield Wiper Blade Inserts (All Models)

- Driver's Side - 21.5 inches (54.6 cm)
- Passenger's Side - 20.0 inches (50.8 cm)

21303407

Spark Plugs: |
- SOHC (L24) Engine | NGK BKR4ESA-11 (Saturn Part No. 21025102) (Gap at 1.0 mm (0.040 in.])
- DOHC (LL0) Engine | NGK BKR5ESA-11 (Saturn Part No. 21025103) (Gap at 1.0 mm [0.040 in.])
DO NOT remove spark plugs from a hot engine. It may cause cylinder head thread damage.

### Tire Loading Information

| OCCUPANTS | VEHICLE CAPACITY WEIGHT
--- | --- | ---
MODEL | FRT | CTR | RR | TOTAL | LBS | KG
SEDAN (SL, SL1, SL2) | 2 | 0 | 3 | 5 | 864 | 392
COUPE (SC1, SC2) | 2 | 0 | 2 | 4 | 714 | 324

MAXIMUM LOADING AT GVWR: SAME AS VEHICLE CAPACITY WEIGHT

### Tire Specification Information

MODEL |  | TIRE SIZE | SPEED RATING** | COLD TIRE PRESSURE PSI/KPA
--- | --- | --- | --- | ---
SEDAN (SL, SL1) | FRT | P185/65 R14 | S | 30/210
COUPE (SC1) | RR | 26/180
SEDAN (SL2) | FRT | P185/65 R15 | T | 30/210
COUPE (SC1)* | RR
COUPE (SC2) | FRT | P195/60 R15 | H | 30/210
RR | P205/50 R16 (If Equipped) | 26/180
ALL | SPARE | T115/70 R14 | M | 60/415
If tires are hot, add 4 PSI (28 kPa)
* SC1 Optional Tire ** Refer to the tire manufacturer's tire warranty booklet, included with this owner's handbook, for an explanation of speed rating and for other important information about your tires.