For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the positive battery cable.
3. Remove the underhood fuse block (UHFB) fasteners.
4. Turn UHFB over and open the fuse block case.
5. Remove the connectors: (1-6).
6. Remove the UHFB from the vehicle.

### Installation Procedure

1. Connect the connectors (1-6) to the fuse block.
2. Route the UHFB harnesses: (A) Forward Lamp, (B) Engine, (C) Instrument Panel into fuse block case.
3. Close and latch the fuse block case.
4. Position the UHFB into place.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the UHFB fasteners.

Tighten
Tighten the underhood fuse block fasteners to 9 N·m (80 lb in).

6. Connect the positive battery cable.
7. Connect the negative battery cable.