For 1990-2009 cars

### Removal Procedure

1. Disable the SIR System. Refer to Disabling the SIR System in SIR.
2. Remove the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
3. Disconnect the park brake switch electrical connector.
4. Remove the park brake switch screw, and remove the switch.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Pull the park brake lever up; place the park brake switch into position. Secure it by installing the park brake switch screw.

Tighten
Tighten the park brake switch screw to 4 N·m (35 lb in).

2. Connect the park brake indicator switch electrical connector.
3. Install the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
4. Enable the SIR System. Refer to Enabling the SIR System in SIR.