For 1990-2009 cars

### Removal Procedure

1. Remove the quarter outer panel. Refer to Quarter Panel Replacement - Bolt On .
2. Remove the fuel cap with the safety strap from the filler pocket.
3. Remove the fuel tank filler pocket by sliding off the fuel filler neck.

### Installation Procedure

1. Install the fuel tank filler pocket over the filler neck.
2. Install the fuel cap and attach the safety strap.
3. Install the quarter outer panel. Refer to Quarter Panel Replacement - Bolt On .