For 1990-2009 cars

### Removal Procedure

1. Remove the screw from center of inside door handle assembly.
2. Slide the door handle assembly forward while pulling outward from the trim panel.
3. Disconnect the electrical connector.
4. Remove the switch from the door handle assembly by releasing the retainer tabs.

### Installation Procedure

1. Install the switch to the door handle assembly.
2. Connect the electrical connector.
3. Position the door handle assembly into the trim panel.
4. Install the screw in the handle and tighten

Notice: Refer to Fastener Notice in the Preface section.

5. Check the operation switch.

Tighten
Tighten the rear door inside release handle fastener to 2.5 N·m (22 lb in).