For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Center High-Mount Stop Lamp (Sedan/Wagon) | 2.5 N·m | 19 lb in
Compartment Deck Lid-to-Hinge Arm | 10 N·m | 89 lb in
Compartment Lid Spoiler | 5 N·m | 44 lb in
Compartment Liftgate, Striker (Wagon) | 25 N·m | 19 lb ft
Fuel Door Latch Retaining Nut | 2 N·m | 18 lb in
Fuel Filler Door Release Handle-to-Floor Fasteners Nut | 2.2-2.3 N·m | 22 lb in
Fuel Filler Door-to-Quarter Panel Fasteners | 2.5 N·m | 22 lb in
Lift Gate Hinge-to-Body Bolts | 10 N·m | 89 lb in
Lift Gate Hinge-to-Hinge Bolts | 10 N·m | 89 lb in
Lift Gate Hinge-to-Liftgate Bolts | 10 N·m | 89 lb in
Lif Ggate Latch-to-Liftgate Fasteners | 10 N·m | 89 lb in
Lift Gate Striker Fasteners | 10 N·m | 89 lb in
Lift Gate Striker Fasteners | 25 N·m | 19 lb ft
Quarter Panel (Sedan) | 9 N·m | 80 lb in
Quarter Panel (Wagon) | 6 N·m | 53 lb in
Rear Bumper Impact Bar Nuts (All Models) | 30 N·m | 22 lb ft
Rear Center Reflex | 5 N·m | 43 lb in
Rear Compartment Deck Lid-to-Hinge Arm | 10 N·m | 89 lb in
Rear Compartment Hinge to Body Nuts | 25 N·m | 19 lb ft
Rear Compartment Interior Release Handle-to-Floor Bolt | 10 N·m | 89 lb in
Rear Compartment Latch Striker Bolts (Sedan/Coupe) | 10 N·m | 89 lb in
Rear Compartment Lid Hinge-to-Rear Window Lower Panel (Sedan/Coupe) | 25 N·m | 19 lb ft
Rear Quarter Panel Attachment Bolts (Coupe) | 9 N·m | 80 lb in
Rear Compartment Lid Latch Bolts | 10 N·m | 89 lb in
Rear Compartment Lid to Hinge Bolt | 10 N·m | 89 lb in
Seat Adjuster-to-Vehicle Bolts | 35 N·m | 26 lb ft
Tail Lamp Assembly (Sedan/Wagon) | 3.5 N·m | 31 lb in
Tail Lamp Assembly (Coupe) | 2.5 N·m | 22 lb in