For 1990-2009 cars

### Removal Procedure

1. Remove pump assembly from vehicle as previously outlined.
2. Remove reservoir retaining clips from reservoir assembly.
3. Remove reservoir from housing.
4. Remove O-ring seal from pump housing.

### Installation Procedure

1. Lubricate new O-ring seal with power steering fluid and install into reservoir.
2. Install reservoir into pump housing. Make sure to push reservoir straight into housing.
3. Install reservoir retaining clips.
4. Install pump into vehicle, as previously described.
5. Bleed power steering system. Refer to Power Steering System Bleeding .