For 1990-2009 cars

### Removal Procedure

1. Remove the lift gate window upper molding retainer.
2. Pull firmly at the attaching clip locations to disengage the clips.
3. Remove the molding.
4. Remove the center high mounted stop lamp (CHMSL) fasteners to remove the CHMSL.
5. Remove the rear washer nozzle attaching clip.
6. Disconnect the rear washer nozzle hose and remove the washer nozzle.

### Installation Procedure

1. Connect the rear washer nozzle hose.
2. Install the rear washer nozzle to the lift gate.
3. Install the rear washer nozzle attaching clip to the nozzle.
4. Install the center high mount stop lamp (CHMSL).
5. Position the lift gate window upper molding to the vehicle.
6. Push at the attaching clip locations to engage the clips.
7. Install the retainers.