For 1990-2009 cars

### Removal Procedure

1. Remove the retaining screws.
2. Slide the applique forward to disengage the hooks from the door.

### Installation Procedure

1. Position the applique on the door; then press on the applique to seat the hooks inside of the applique into the slots in the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the retaining screws.

Tighten
Tighten the rear door front applique screws (Sedan/Wagon) to 2 N·m (18 lb in).